HOW TO INSTALL THE SOFTWARE UPDATE
==================================
Extract all the files contained in the compressed ZIP file to the root (top 
level) of an empty, FAT32 formatted, USB Stick.

From any Target Unit with Software Running
------------------------------------------ 
Insert the USB Stick into the USB Port of a running target unit and the update 
process will begin. There will be on-screen information during the update 
process. Please remove the USB Stick when prompted and the target unit will 
automatically reboot into the new software.

From a 3.5" Target Unit that Won't Boot
--------------------------------------- 
Make sure the power is off then insert the USB Stick into the USB Port. Turn 
on the power while simultaneously holding down Key1 and Key5. The screen will 
turn blue and after a few seconds the update process will begin. There will be 
on-screen information during the update process. Please remove the USB Stick 
when prompted and the target unit will automatically reboot into the new 
software.

From a 7" Target Unit that Won't Boot
------------------------------------- 
Make sure the power is off then insert the USB Stick into the USB Port. Turn 
on the power while simultaneously holding down the small red button right next 
to the USB port on the back of the unit. The screen will turn blue and after a 
few seconds the update process will begin. There will be on-screen information 
during the update process. Please remove the USB Stick when prompted and the 
target unit will automatically reboot into the new software.

KNOWN ISSUES
============
Some USB Sticks are not compatible with the target unit. If the update does 
not install properly, please try a different type of USB Stick.

If the problems persist, please contact Techinical Support for more help.
